**EXPERIMENT-6**

**IMPLEMENTATION OF TREE TOPOLOGY USING PACKET**

**TRACER**

**Aim:** To Implement a tree topology using packet tracer and hence to transmit data

between the devices connected using tree topology.

**Software / Apparatus required:** Packet Tracer / End devices, Hubs, connectors.

**Procedure:**

**Steps for building topology:**

**Step 1: Start Packet Tracer**

**Step 2: Choosing Devices and Connections**

**Step 3: Building the Topology – Adding Hosts**

Single click on the **End Devices**.

Single click on the **Generic** host.

Move the cursor into topology area.

Single click in the topology area and it copies the device.

**Step 4: Building the Star Topology – Connecting the Hosts to Hubs**

Select a Hub, by clicking once on **Hub** and once on a **generic Hub**

Add the Hub by moving the plus sign “**+**”

**Step 5: Connect PCs to Hub by first choosing Connections**

Click once on the **Automatic cable selector**

Click once on **PC2**

Choose **Fast Ethernet**

Drag the cursor to **Hub0**

Click once on **Hub0**

**Proceeding in this way create three star topologies**

**Step 6: Building the Tree Topology – Connecting the Hubs to Active Hub**

Connect the hubs of star topologies to active hub to create tree topology.

**Step 7: Configuring IP Addresses and Subnet Masks on the Hosts**

To start communication between the hosts IP Addresses and Subnet Masks had to be

configured on the devices. Click once on PC0. Choose the Config tab and click on

Fast Ethernet0. Type the IP address in its field. Click on the subnet mask. It will begenerated automatically.

**Step 8: Verifying Connectivity in Real time Mode**

Be sure you are in **Real time** mode.

Select the **Add Simple PDU** tool used to ping devices.

Click once on PC0, then once on PC3.

The PDU **Last Status** should show as **Successful**.

**Step 9:** **Verifying Connectivity in Simulation Mode**

Be sure you are in **Simulation** mode.

Deselect all filters (All/None) and select only **ICMP**.

Select the **Add Simple PDU** tool used to ping devices


Click once on PC0, then once on PC3.

Continue clicking **Capture/Forward** button until the ICMP ping is completed.


You should see the ICMP messages move between the hosts, hub and switch. The

PDU **last status** should show as **Successful**.

**Diagram:**



**Output:**



**Result:** Thus the Tree topology is implemented with Packet Tracer simulation Tool.